<60F-W0>[ka] = cq de hb9htc = ge dr yl, swl es om. Es folgt das Morsetraining des htc, helvetia telegraphy club, Uebung Nr. 50 = nw Tempo 45/9 wpm<45F60W3000> <W0>= Unter ganz verschiedenen Umstaenden, wer weiss warum? = tn/6q q0'pa (iji) = We all had a grand time, and it was nice to spend the time with you and Silvia. = Jdtuj gdjrb bluil ffjbr + de hb9htc = nw Tempo 60/12 wpm<60F-W3000> <W0>= swsmj dkkfh lilwy nvztu tzgqb 53051 50315 wreqj = die Fortsetzung folgt = Next it will be our turn for revenge. = Am Muttertag hatten wir ein schoenes Erlebnis. Morgens um 8 Uhr wurde ein ofenfrischer Zopf ins Haus geliefert. = Was ist SWR? Betrachten wir uns die Leitung L naeher. = The decree shall be reconsidered and the person shall not. + de hb9htc = nw Tempo 80/16 wpm<80W3000> <W0>= If a bipolar transistor is used as the active element in a VFO, it should have an ft considerably higher than tho VFO operating frequency, say, a 250 MHz ft for a 7 MHz = oscs1 tp34/ wkjji m.p-x yyzqe a1/b. sv9ga hb9rf hb9jo hb9qu. = Surtout les bons commutateurs de puissance HF avec les galettes en ceramique + de hb9htc = nw Tempo 100/20 wpm<100W3000> <W0>= also hope you had a fun and successful time at H26. Although I personally didn't work HB9HTC, I heard we got you on a couple of bands. = mi38n zu05t gvn98765 12345 = Bei den meisten Om's wird dazu ein Koaxialkabel mit 50 ohm Wellenwiderstand verwendet, weniger eine Paralleldrahtleitung. = mni tks abt info cuagn pse psed = Open wire line, Coaxial line, equivalent circuit of balanced line, Generator, Load. + de hb9htc = nw Tempo 120/24 wpm<120W3000> <W0>= I wanted to tell you about our May 1 excursion to the vineyards. We decided to go up to the region near Eglisau, and our photocopied map was a great help. = 554t4 p3r(b) ?/x?/ 73f5h 6nm13 efkij o0739 = We started at the Schloss in Teufen and that was very nice. Marge joked that he hoped we hadn't peaked too early, but as the rest of the day showed, we in fact had. = Equivalent cicuit to balanced line. = Nun transportiert diese Leitung aber nicht Gleichstrom sondern HF. In der tat - so ist es. + de hb9htc = nw Tempo 140/28 wpm<140W3000> <W0>= EUCW AGCW UFT HTC VHSC HSC INORC OECWG YLCWG = We hiked to Toessegg and took the little ferry boat across the Rhine and at the other shore saw the bell you ring for service. Then we hiked to Eglisau and shopped at a small winery - not much to see, but we did enjoy some wine. In all, according to Marge's pedometer, we marched 25,000+ paces, and we were good and tired when we got home. But all in all, it was a pleasant day. = Hast Du heute schon mal gelacht? Ja - gut so, nein - dann ist es Zeit, das nachzuholen. Am besten lachst Du jetzt ueber dich selbst. Was, du hast keinen Grund dazu? + de hb9htc <60W3000> <W0>= Das war das woechentliche Morsetraining des htc, Uebung Nr. 50 = dr op, cuagn next Monday = 73 de hb9htc.ch [ar]